|  |  |  |  |
| --- | --- | --- | --- |
| **Line** | **R12** | **R13** | **Purpose** |
| 66 | #NOKIA\_DATA | 0xE7 | Draw an 8 pixel high line and beam with a 2 pixel hole in the center |
| 276 | #NOKIA\_CMD | R12 | Sends the row (page) address |
| 288 | #NOKIA\_CMD | R12 modified to location | Sends the upper and lower columns with the address shifted right 4 bits |
| 294 | #NOKIA\_CMD | R13 & 0x0F | Makes a copy to the top of the stack |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Line** | | **Command/Data** | **8-Bit Packet** | |
| 66 | | Data | 11100111 | |
| 276 | | Command | 10110001 | |
| 288 | Command | | | 00010000 |
| 294 | Command | | | 00000001 |